**OPCIONES FABRICACIÓN jlcpcb.com**

* **Layers:** 4 capas
* **Dimensions:** 50 \* 50 mm
* **PCB Qty:** 5
* **Different Design:** 1
* **Delivery Format:** Single PCB
* **PCB Thickness:** 1mm
* **PCB Color:** Black
* **Text Color:** White
* **Surface Finish:** HASL (with lead)
* **Copper Weight:** 1 oz
* **Gold Fingers:** No
* **Confirm Production file:** No
* **Flying Probe Test:** Fully Test
* **Castellated Holes:** No
* **Remove Order Number:** No